{"text_format":"5","workbook":"xls","n_sheets":3,"sheets":["Arkusz1","Arkusz2","Arkusz3"],"props":{"creator":"beata","last_modified_by":"rendanis","company":"imid"},"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Arkusz1","index":0,"n_rows":9,"n_cols":10,"rows_kept":9,"merged":[[1,7,1,9],[3,0,3,9],[4,1,4,9],[8,0,8,4],[10,3,10,9],[11,6,11,9],[12,6,13,9]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":7},"Załącznik nr 2 do zapytania ofertowego"]
[]
["TABELA ASORTYMENTOWO-CENOWA"]
[]
[]
["Lp.","Nazwa przedmiotu zamówienia","J.m.","Ilość   ","Cena jedn. netto            w PLN","Wartość netto w PLN","Stawka VAT","Wartość brutto w PLN","Producent/ Model proponowanego urządzenia","Nr katalogowy "]
[1,"Głowica dozująca odpowiednia do stacji pipetującej epMotion przeznaczona do zautomatyzowanego przygotowania bibliotek NGS. Jednokanałowa, obiętość dozowania 0,2 – 10 μL; bezwzględny błąd systematyczny pipetowania w granicach od +0,05 μL do +0,12 μL","szt.",1]
["RAZEM:"]

{"sheet":"Arkusz2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"Arkusz3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}